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GUIDELINES


GENERAL INFORMATION
The ILC scheme, titled "Interlaboratory tests on cement", meets the requirements of the                                      EN ISO/IEC 17043 standard: “Conformity assessment. General requirements for proficiency testing”. Participation is confidential, and each laboratory receives a unique code number every year.
Once the statistical calculations of the results are completed, each participant will receive a General Report containing the evaluation of the results based on the “z”-score.
The cement samples provided to participants by CEPROCIM S.A. must be tested by ALL participants between 2 and 13 November 2026, in accordance with the following instructions:
• The cement must be tested on the same day the container is opened.
• Before performing the tests, the total quantity of cement enclosed in the container must be homogenized to properly remix any components that may have segregated over time during transport.

INFORMATION REGARDING THE TESTS
All participants in the scheme must use the cement received in the package. The sand used should be specific to each participating laboratory.
As cement has a high tendency to agglomerate, thorough homogenization of the sample is mandatory prior to testing.
The tests included in the scheme comply with EN 196-1, EN 196-2, BS EN 196-2:1995, EN 196-3, EN 196-6 and EN 196-10.
	The test results must be entered on the RESULTS FORM and sent by e-mail or fax to CEPROCIM S.A. no later than 18 December 2026.






CONTACT:
Nicoleta VLAD, e-mail: nicoleta.vlad@ceprocim.ro
Cristina STANCU, e-mail: cristina.stancu@ceprocim.ro



	Organization name:
	

	Contact person:
	

	e-mail:
	



RESULTS FORM
	TEST
	U.M.
	VALUE

	L.O.I. (Loss on ignition), according EN 196-2
	%
	

	SiO2, according EN 196-2
	%
	

	Al2O3, according EN 196-2
	%
	

	Fe2O3, according EN 196-2
	%
	

	CaO, according EN 196-2
	%
	

	MgO, according EN 196-2
	%
	

	SO3, according EN 196-2
	%
	

	Free CaO, according BS EN 196-2:1995
	%
	

	Ins. Res. in HCl and Na2CO3, according EN 196-2
	%
	

	Na2O, according EN 196-2
	%
	

	K2O, according EN 196-2
	%
	

	Cl-, according EN 196-2
	%
	

	Cr6+, according EN 196-10
	%
	

	Residue on the 90 µm sieve, according EN 196-6
	%
	

	Density, according EN 196-6
	g/cm³
	

	Specific surface area, according EN 196-6
	cm²/g
	

	Standard consistence, according EN 196-3
	%
	

	Initial setting time, according EN 196-3
	min.
	

	Final setting time, according EN 196-3
	min.
	

	Soundness (with Le Chatelier needles), according EN 196-3
	mm
	

	2-days Flexural strength, according EN 196-1
	MPa
	

	7-days Flexural strength, according EN 196-1
	MPa
	

	28-days Flexural strength, according EN 196-1
	MPa
	

	2-days Compressive strength, according EN 196-1
	MPa
	

	7-days Compressive strength, according EN 196-1
	MPa
	

	28-days Compressive strength, according EN 196-1
	MPa
	



LABORATORY MANAGER
Name, surname



NOTE: All participants must test the sample between 2 and 13 November 2026.
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